| **Name** | **Description** | **Read/Write** | **Hex Addr** | **Dec Addr** | **Shadow Name** | **Shadow Hex Addr** | **Shadow Dec Addr** |
| --- | --- | --- | --- | --- | --- | --- | --- |
| [AUDF1](https://en.wikipedia.org/wiki/POKEY#AUDF1_$D200_Write) | Audio Channel 1 Frequency | Write | $D200 | 53760 |  |  |  |
| [POT0](https://en.wikipedia.org/wiki/POKEY#POT0_$D200_Read) | Potentiometer (Paddle) 0 | Read | $D200 | 53760 | PADDL0 | $0270 | 624 |
| [AUDC1](https://en.wikipedia.org/wiki/POKEY#AUDC1_$D201_Write) | Audio Channel 1 Control | Write | $D201 | 53761 |  |  |  |
| [POT1](https://en.wikipedia.org/wiki/POKEY#POT1_$D201_Read) | Potentiometer (Paddle) 1 | Read | $D201 | 53761 | PADDL1 | $0271 | 625 |
| [AUDF2](https://en.wikipedia.org/wiki/POKEY#AUDF2_$D202_Write) | Audio Channel 2 Frequency | Write | $D202 | 53762 |  |  |  |
| [POT2](https://en.wikipedia.org/wiki/POKEY#POT2_$D202_Read) | Potentiometer (Paddle) 2 | Read | $D202 | 53762 | PADDL2 | $0272 | 626 |
| [AUDC2](https://en.wikipedia.org/wiki/POKEY#AUDC2_$D203_Write) | Audio Channel 2 Control | Write | $D203 | 53763 |  |  |  |
| [POT3](https://en.wikipedia.org/wiki/POKEY#POT3_$D203_Read) | Potentiometer (Paddle) 3 | Read | $D203 | 53763 | PADDL3 | $0273 | 627 |
| [AUDF3](https://en.wikipedia.org/wiki/POKEY#AUDF3_$D204_Write) | Audio Channel 3 Frequency | Write | $D204 | 53764 |  |  |  |
| [POT4](https://en.wikipedia.org/wiki/POKEY#POT4_$D204_Read) | Potentiometer (Paddle) 4 | Read | $D204 | 53764 | PADDL4 | $0274 | 628 |
| [AUDC3](https://en.wikipedia.org/wiki/POKEY#AUDC3_$D205_Write) | Audio Channel 3 Control | Write | $D205 | 53765 |  |  |  |
| [POT5](https://en.wikipedia.org/wiki/POKEY#POT5_$D205_Read) | Potentiometer (Paddle) 5 | Read | $D205 | 53765 | PADDL5 | $0275 | 629 |
| [AUDF4](https://en.wikipedia.org/wiki/POKEY#AUDF4_$D206_Write) | Audio Channel 4 Frequency | Write | $D206 | 53766 |  |  |  |
| [POT6](https://en.wikipedia.org/wiki/POKEY#POT6_$D206_Read) | Potentiometer (Paddle) 6 | Read | $D206 | 53766 | PADDL6 | $0276 | 630 |
| [AUDC4](https://en.wikipedia.org/wiki/POKEY#AUDC4_$D207_Write) | Audio Channel 4 Control | Write | $D207 | 53767 |  |  |  |
| [POT7](https://en.wikipedia.org/wiki/POKEY#POT7_$D207_Read) | Potentiometer (Paddle) 7 | Read | $D207 | 53767 | PADDL7 | $0277 | 631 |
| [AUDCTL](https://en.wikipedia.org/wiki/POKEY#AUDCTL_$D208_Write) | Audio Control | Write | $D208 | 53768 |  |  |  |
| [ALLPOT](https://en.wikipedia.org/wiki/POKEY#ALLPOT_$D208_Read) | Read 8 Line POT Port State | Read | $D208 | 53768 |  |  |  |
| [STIMER](https://en.wikipedia.org/wiki/POKEY#STIMER_$D209_Write) | Start Timers | Write | $D209 | 53769 |  |  |  |
| [KBCODE](https://en.wikipedia.org/wiki/POKEY#KBCODE_$D209_Read) | Keyboard Code | Read | $D209 | 53769 | CH | $02FC | 764 |
| [SKREST](https://en.wikipedia.org/wiki/POKEY#SKREST_$D20A_Write) | Reset Serial Status (SKSTAT) | Write | $D20A | 53770 |  |  |  |
| [RANDOM](https://en.wikipedia.org/wiki/POKEY#RANDOM_$D20A_Read) | Random Number Generator | Read | $D20A | 53770 |  |  |  |
| [POTGO](https://en.wikipedia.org/wiki/POKEY#POTGO_$D20B_Write) | Start POT Scan Sequence | Write | $D20B | 53771 |  |  |  |
| [SEROUT](https://en.wikipedia.org/wiki/POKEY#SEROUT_$D20D_Write) | Serial Port Data Output | Write | $D20D | 53773 |  |  |  |
| [SERIN](https://en.wikipedia.org/wiki/POKEY#SERIN_$D20D_Read) | Serial Port Data Input | Read | $D20D | 53773 |  |  |  |
| [IRQEN](https://en.wikipedia.org/wiki/POKEY#IRQEN_$D20E_Write) | Interrupt Request Enable | Write | $D20E | 53774 | POKMSK | $10 | 16 |
| [IRQST](https://en.wikipedia.org/wiki/POKEY#IRQST_$D20E_Read) | IRQ Status | Read | $D20E | 53774 |  |  |  |
| [SKCTL](https://en.wikipedia.org/wiki/POKEY#SKCTL_$D20F_Write) | Serial Port Control | Write | $D20F | 53775 | SSKCTL | $0232 | 562 |
| [SKSTAT](https://en.wikipedia.org/wiki/POKEY#SKSTAT_$D20F_Read) | Serial Port Status | Read | $D20F | 53775 |  |  |  |